This release includes iavf Linux* Virtual Function Drivers for
Intel(R) Ethernet Network Connections.

The iavf driver supports devices based on the following controllers:

* Intel(R) Ethernet Controller I710

* Intel(R) Ethernet Controller V710

* Intel(R) Ethernet Controller X710

* Intel(R) Ethernet Controller XL710

* Intel(R) Ethernet Controller XXV710

* Intel(R) Ethernet Network Connection X722

* Intel(R) Ethernet Controller E810-C

* Intel(R) Ethernet Controller E810-XXV

* Intel(R) Ethernet Connection E822-C

* Intel(R) Ethernet Connection E822-L

* Intel(R) Ethernet Connection E823-C

* Intel(R) Ethernet Connection E823-L

* Intel(R) Ethernet Controller E830

iavf-x.x.x.tar.gz

Due to the continuous development of the Linux kernel, the drivers are
updated more often than the bundled releases. The latest driver can be
found at the following locations:

* http://downloadcenter.intel.com

* https://github.com/intel/ethernet-linux-iavf

This release includes RPM packages that contain:

* Device driver signed with Intel's private key in precompiled kernel
  module form

* RDMA driver

* Complete source code for above drivers

* Intel's public key

This release includes the Intel public key to allow you to
authenticate the signed driver in secure boot mode. To authenticate
the signed driver, you must place Intel's public key in the UEFI
Secure Boot key database.

Note:

  * The driver kernel module for a specific kernel version can be used
    with errata kernels within the same minor OS version, unless the
    errata kernel broke kABI. Whenever you update your kernel with an
    errata kernel, you must reinstall the driver RPM package.

  * The RDMA driver will be installed if you reinstall the driver RPM
    package. If you want to remove the RDMA driver, you will have to
    do so every time you install the RPM package (for example, when
    you update your kernel with an errata kernel).

  * If you decide to recompile the .ko module from the provided source
    files, the new .ko module will not be signed with any key. To use
    this .ko module in Secure Boot mode, you must sign it yourself
    with your own private key and add your public key to the UEFI
    Secure Boot key database.
